For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove rear side door trim panel. Refer to Rear Side Door Trim Replacement.

1 | Rear Side Door Check Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Place the door in the full open position. Tighten
25 N·m(18 lb ft)

2 | Rear Side Door Check Nut

#### Procedure

Remove the water deflector.

Tighten
9 N·m(79 lb in)

3 | Rear Side Door Check