For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 2-6 Clutch Piston Assembly Tip

• | Position the 2-6 piston air bleed and large slot toward the top of the case.

• | DT-47796 seal protector prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of the DT-47796 seal protector to ease installation of the piston.

#### Special Tool

DT-47796 Seal Protector

For equivalent regional tools, refer to Special Tools.

2 | 2-6 Clutch Spring
3 | 2-6 Clutch Spring Retainer Caution: Regulate the air pressure to 40 psi maximum. High pressure could cause the piston to over travel and damage the piston seals. Tip

• | Place the retainer on the 2-6 clutch spring and align the retainer opening with the largest gap in the case splines toward the bottom of the case. The retainer opening should be supported by a spline tooth of the case.

• | Apply shop air to the clutch fluid feed hole in the case to verify proper piston operation.

#### Special Tools

• | DT-47797 Spring Installer

• | DT-48056 Spring Compressor Bridge

For equivalent regional tools, refer to Special Tools.