For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the generator and air conditioning compressor belt. Refer to Drive Belt Replacement.
3. Remove the drive belt tensioner bolt (2).
4. Remove the drive belt tensioner (1).

### Installation Procedure

1. Clean the drive belt tensioner thread.
2. Install drive belt tensioner (1).

Caution: Refer to Fastener Caution in the Preface section.

3. Install drive belt tensioner bolt (2) and tighten to 50 N·m (37 lb ft).
4. Install the generator and air conditioning compressor belt. Refer to Drive Belt Replacement.
5. Close the hood.