For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear side door trim panel. Refer to Rear Side Door Trim Replacement.
2. Remove the rear side water deflector. Refer to Rear Side Door Water Deflector Replacement.
3. Remove the rear door window outer sealing strip. Refer to Rear Side Door Window Outer Sealing Strip Replacement.
4. Remove the rear side door window. Refer to Rear Side Door Window Replacement.

1 | Rear Side Door Stationary Window Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten xx N·m (xx lb ft)
2 | Rear Door Stationary Window

#### Procedure

Pull the bulb straight from the lamp harness socket.