For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel lower trim pad cover. Refer to Instrument Panel Lower Trim Pad Cover Replacement.

1 | Brake Pedal Position Sensor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Brake Pedal Position Sensor

#### Procedure

1. Disconnect the electrical connector.
2. Calibrate the brake pedal position sensor. Refer to Brake Pedal Position Sensor Calibration.