For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove as much power steering fluid from the remote power steering fluid reservoir as possible.
2. Place drain pans under the vehicle as needed.

1 | Power Steering Gear Inlet Hose Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 11 N·m (98 lb in).
2 | Hose Clamp

#### Procedure

Compress the power steering fluid reservoir outlet hose clamp from the power steering fluid reservoir.

3 | Power Steering Gear Outlet Hose

#### Procedure

Fill and bleed the power steering system. Refer to Power Steering System Bleeding.

Tip
Clean any excess power steering fluid from the vehicle.