For 1990-2009 cars

Checks | Causes
--- | ---
Low-Reverse and 1-2-3-4 Clutch Housing (551) |

• | Inspect for damaged or broken 1-2-3-4 Clutch Piston (552) and piston seals damaged, worn or leaking

• | Inspect for fatigued or binding 1-2-3-4 Clutch Piston Return Spring (553)

• | Inpsect for improper surface finish on 1-2-3-4 Clutch Plates (557-559)

• | Inspect for broken or fatigued 1-2-3-4 Clutch Waved Plate (557)

• | Inspect for plugged or restricted Low-Reverse and 1-2-3-4 Clutch Piston Housing (551) air bleed

Case Assembly (50) |

• | Inspect for leaking or loose fitting Fluid Check Valve (55)

• | Inspect for leaking or damaged 1-2-3-4 and Low-Reverse Clutch Fluid Passage Seals (67)