For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear compartment sill trim plate. Refer to Rear Compartment Sill Trim Plate Replacement.
2. Disconnect the electrical harness connector from the backup lamp socket.

1 | Back Up Lamp Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb ft)
2 | Back Up Lamp Assembly Warning: Refer to Glass and Sheet Metal Handling Warning in the Preface section. Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Reach inside the rear compartment lid inner panel and remove the lower and upper retainer nuts securing the lamp assembly to the outer rear compartment lid panel.
2. Push the inside edge of the lamp assembly outward from the rear outer compartment lid panel.
3. Remove and transfer the bulb socket from the back up lamp assembly.