For 1990-2009 cars

#### Special Tools

• | EN-48253 Accessory Belt Remover

• | EN-48952 Tensioner Spring Holding Pin

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement.
2. Remove the drive belt tensioner bolt (2).
3. Remove the drive belt tensioner (1).

### Installation Procedure

1. Install the drive belt tensioner (1).

Caution: Refer to Fastener Caution in the Preface section.

Note:

• | The tensioner dowel pin (a) is not aligned with the tensioner dowel pin hole (b) at this stage.

• | Tightening the bolt will damage the tensioner and the tensioner dowel pin.

2. Install the drive belt tensioner bolt (2) and tighten to 52 N·m (39 lb ft).
3. Install the drive belt. Refer to Drive Belt Replacement.