For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Disconnect electrical connector.

1 | Air Inlet Valve Actuator Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (23 lb in)
2 | Air Inlet Valve Actuator

#### Procedure

Calibration instructions. Refer to Actuator Recalibration.

Tip
The graphic shows air inlet valve actuator without instrument panel for better clarity.