For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

Note: DO NOT re-use the lower ball joint bolt. Discard and use NEW only.

3. Remove wheel speed sensor wiring harness from control arm and steering knuckle.
4. Remove the lower ball joint to knuckle nut and bolt (1).
5. Separate the lower control arm from the knuckle.
6. Remove the front lower control arm nut and bolt (1).
7. Remove the rear lower control arm bushing nuts and bolts (1).
8. Remove the lower control (1) arm from the front frame.

### Installation Procedure

1. Position the lower control arm (1) in the cradle.
2. Install and hand tighten the rear lower control arm bushing nuts and bolts (1).
3. Install and hand tighten the front lower control arm nut and bolt.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the ball joint to knuckle bolt and nut and tighten to XX N·m (xx lb ft).
5. Load the front suspension with the proper jack stand before tightening the bolts to specifications.
6. Tighten the front lower control arm bolt to XX N·m (xx lb ft).
7. Tighten the rear bushing to frame bolts to XX N·m (xx lb ft).
8. Remove the jack stand.
9. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
10. Lower the vehicle.