For 1990-2009 cars

### Exterior Lamps

The exterior lighting system consist of the following lamps:

• | Headlamps

• | Front fog lamps

• | Park, tail and license lamps

• | Turn signal lamps

• | Hazard warning lamps

• | Repeater lamps

• | Stop lamps

• | Backup lamps

• | Position lamps

### Low Beam Headlamps

The headlamps consist of 2 interchangeable single filament bulbs or 2 high intensity discharge (HID) arc tubes and ballast on each side of the vehicle which provide high and low beams. The lower bulb in the headlamp is the high beam and the upper bulb is the low beam.

The headlamps may be turned ON in 3 different ways:

• | When the headlamp switch is placed in the ON position, for normal operation

• | When the headlamp switch is placed in the AUTO position, for automatic lamp control

• | When the headlamp switch is placed in the AUTO position, with the windshield wipers ON in daylight conditions, after a 6 s delay

The body control module (BCM) controls the headlamps based on the inputs explained above. When a low beam request is received, the BCM supplies an B+ through the headlamp low beam relay for the left headlamp and through daytime running lamp relay - right for the right headlamp. This then applies B+ to the low beam headlamps, illuminating the low beam headlamps. When a high beam request is received, the BCM grounds the headlamp high beam relay control circuit. This energizes the coil in the headlamp high beam relay, causing the relay switch to close. This then applies B+ to both high beam headlamps through the left high beam and right high beam fuses, illuminating the high beam headlamps.

### Automatic Lamp Control

Automatic Light is switched on as default. It can be switched off by turning the light switch to OFF position. It will be switched on again by doing so again. Automatic Light is only available if a rain sensor or rain/light sensor module (RSM) in installed in the car. RSM will send the actual ambient light state (day/night) to the BCM. If Automatic Light is enabled, BCM will react on the message received from RSM by switching ON/OFF low beams.

### Flash to Pass

When the low beam headlamps are on and the turn signal/multifunction switch is momentarily placed in the flash to pass position, ground is applied to the turn signal/multifunction switch. The turn signal/multifunction switch applies ground to the BCM through the flash to pass switch signal circuit. The BCM then applies ground to the high beam relay control circuit. This energizes the high beam relay, closing the switch side contacts of the high beam relay, applying battery voltage to the left and right high beam fuses. Battery voltage is applied from the high beam fuses through the high beam voltage supply circuit to the high beam headlamp assemblies. This causes the high beam headlamps to illuminate at full brightness momentarily or until the flash to pass switch is released.

### Front Fog Lamps

The rear fog lamp switch signal circuit is grounded momentarily by pressing the rear fog lamp switch. The BCM energizes the rear fog lamp supply voltage circuit which illuminates the rear fog lamp. With the rear fog lamp switch activated the BCM sends a message via serial data to the instrument panel cluster requesting the instrument panel cluster to illuminate the rear fog indicator.

### Park, Tail and License Lamps

The park lamps, tail lamps/LEDs and number plate lights are turned ON when the headlamp switch is placed in the Parking lights or Low beam position or anytime the headlights are requested. When the BCM receives a request from the headlamp switch to turn ON the park lamps the BCM a sends out a PWM signal, which illuminates the park lamps, tail lamps and number plate lights.

### Turn Signal Lamps

Ground is applied at all times to the turn signal/multifunction switch. The turn signal lamps may only be activated with the ignition switch in the ON or START position. When the turn signal/multifunction switch is placed in either the TURN RIGHT or TURN LEFT position, ground is applied to the BCM through either the right turn or left turn signal switch signal circuit. The BCM then applies a pulsating voltage to the front and rear turn signal lamps through there respective voltage supply circuits. When a turn signal request is received by the BCM, a serial data message is sent to the instrument cluster requesting the respective turn signal indicator be pulsed ON and OFF.

### Repeater Lamps

The repeater lamps are located in the front fender. The repeater lamps are used as additional turn signal lamps, and operate as described in the Turn Signal/Hazard Flasher Lamps description.

### Hazard Flasher Lamps

The hazard flashers may be activated in any power mode. The hazard switch is permanently grounded. When the hazard switch is placed in the ON position, ground is applied through the hazard switch signal circuit to the BCM. The BCM supplies battery voltage to all turn signal lamps in an ON and OFF duty cycle. When the hazard switch is activated, the BCM sends a serial data message to the instrument cluster requesting both turn signal indicators to be cycled ON and OFF.

### Stop Lamps

The brake pedal position (BPP) sensor is used to sense the action of the driver application of the brake pedal. The BPP sensor provides an analog voltage signal that will increase as the brake pedal is applied. The BCM provides a low reference signal and a 5 V reference voltage to the BPP sensor. When the variable signal reaches a voltage threshold indicating the brakes have been applied, the BCM will apply battery voltage to the stop lamp control circuit and center high mounted stop lamp control circuit . When the control circuit is energized the stop lamps are illuminated.

### Backup Lamps

When the transmission is placed in the reverse position, the engine control module (ECM) sends a serial data message to the BCM. The message indicates that the gear selector is in the reverse position. The BCM applies battery voltage to the backup lamps. The backup lamps are permanently grounded. Once the driver moves the gear selector out of the reverse position, a message is sent by the ECM via serial data requesting the BCM to remove battery voltage from the backup lamp control circuit.

### Battery Run Down Protection/Inadvertent Power

To provide battery run down protection, the exterior lamps will be deactivated automatically under certain conditions. The BCM monitors the state of the headlamp switch. If the park or headlamp switch is ON when the ignition switch is placed in either the CRANK or RUN position and then placed in the OFF position, the BCM initiates a 10 min timer. At the end of the 10 min, the BCM will turn off the control power output to the park and headlamp relay coils, deactivating the exterior lamps. This feature will be cancelled if any power mode other than OFF becomes active. The BCM will disable battery run down protection if any of the following conditions exist. The park or headlamp switch is placed in the ON to OFF position, and back to the ON position during battery run down protection. The BCM determined that the park or headlamp switch was not active when the ignition was turned OFF.