For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Any time service is being performed which requires removal of the air cleaner assembly, always cover the throttle body opening. This will prevent any foreign material from entering the engine.
1 | Air Cleaner Outlet Duct to Air Cleaner Housing Cover Clamp Caution: Refer to Fastener Caution in the Preface section. Tighten: 3.5 N·m (31 lb in)
2 | Air Cleaner Outlet Duct
3 | Air Cleaner Outlet Duct to Intake Manifold Clamp Tighten: 3.5 N·m (31 lb in)