For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the left outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.

1 | Instrument Panel Lower Trim Pad Cover Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m(X lb in)
2 | Instrument Panel Lower Trim Pad Cover Assembly

#### Procedure

1. Remove headlamp switch.
2. Disconnect the electrical connectors.
3. When replacing the lower trim pad cover, transfer all necessary components.