For 1990-2009 cars

### Removal Procedure

1. Remove the timing belt. Refer to Timing Belt Replacement.
2. Remove the timing belt idler pulley bolt (2).
3. Remove the timing belt idler pulley (2).

### Installation Procedure

1. Clean the timing belt idler pulley thread.

Caution: Refer to Fastener Caution in the Preface section.

Note: Use an assembly tool.

2. Install the timing belt idler pulley and tighten the NEW bolt to 25 N·m (19 lb ft).
3. Install the timing belt. Refer to Timing Belt Replacement.