For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Differential Carrier Baffle
2 | Front Differential Carrier Baffle Bolt M6 x 16 (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (106 lb in)
3 | Drive Link Lube Scoop Seal
4 | Drive Link Lube Fluid Seal
5 | Drive Link Lube Scoop
6 | Driven Sprocket Bearing Assembly
7 | Drive Sprocket Bearing Assembly
8 | Driven Sprocket Assembly, Drive Sprocket Assembly and Drive Link Tip

• | Install the drive link with the colored links and/or part number facing up.

• | The drive link, drive, and driven sprocket assemblies must be installed at the same time.

• | The ball bearing should spin freely and smoothly.

• | The driven sprocket ball bearing inner race has a slight interference fit with the case. Tap gently with the palm of a hand or a soft tip hammer to install.

9 | Park Pawl
10 | Park Pawl Spring
11 | Park Pawl Shaft Tip Check to ensure that the park pawl operates freely and is not binding.