For 1990-2009 cars

#### Special Tools

• | DT-45201 Cooler Line Seal Remover

• | DT-49101 Seal Installer

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Remove the manual shaft and position switch assembly. Refer to Manual Shift Detent Lever with Shaft Position Switch Assembly Replacement.
3. Remove the manual shaft seal using DT-45201 seal remover .

### Installation Procedure

1. Install the manual shaft and position switch assembly. Refer to Manual Shift Detent Lever with Shaft Position Switch Assembly Replacement
2. Install the manual shaft seal using DT-49101 seal installer .
3. Install the battery tray. Refer to Battery Tray Replacement.