For 1990-2009 cars

Warning: Refer to Brake Dust Warning in the Preface section.

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement.
2. Remove partially the rear floor carpet. Refer to Front Floor Panel Carpet Replacement.
3. Remove the parking brake cable (2) from the parking brake lever (1).
4. Remove the parking brake cable from the parking brake cable bracket (3).
5. Remove the parking brake cable clip (1).
6. Remove the parking brake cable grommet (2).
7. Remove the parking brake cable casing retainer bolt (1).
8. Unclip the parking brake cable.
9. Remove the parking brake cable from the rear brake caliper.

### Installation Procedure

1. Install the parking brake cable to the rear brake caliper.
2. Clip in the parking brake cable (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the parking brake cable casing retainer bolt (1). Tighten the bolt XX N·m (XX lb ft).
4. Install the parking brake cable grommet (2).
5. Install the parking brake cable clip (1).
6. Install the parking brake cable to the parking brake cable bracket (3).
7. Install in the parking brake cable (2) to the parking brake lever (1).
8. Install the rear floor carpet. Refer to Front Floor Panel Carpet Replacement.
9. Install the front floor console. Refer to Front Floor Console Replacement.