For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove fuel tank filler door. Refer to Fuel Tank Filler Door Replacement.
2. Drain fuel tank if necessary. If the fuel level is over half filled. Refer to Fuel Tank Draining.
3. Remove rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.
4. Remove fuel tank filler pipe housing. Refer to Fuel Tank Filler Pipe Housing Replacement.

1 | Fuel Tank Filler Pipe Bracket Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Fuel Tank Filler Pipe Ground Bolt Tighten 9 N·m (80 lb in)
3 | Fuel Tank Filler Pipe Clamp
4 | Lower Recirculation Tube Quick Release Fitting
5 | Fuel Tank Filler Pipe Tip Rear suspension and rear axle have been removed for better pictorial illustration.