For 1990-2009 cars

#### Special Tool

CH-804 Drive Axle Seal Clamp Pliers

### Removal Procedure

1. Remove the steering linkage outer tie rod. Refer to Steering Linkage Outer Tie Rod Replacement.
2. Remove the steering linkage inner tie rod nut (1).
3. Remove the steering gear outer boot clamp (2).
4. Loosen the steering gear inner boot clamp (1).
5. Remove the steering gear boot (1).

Note: After removing the boot, inspect the steering linkage inner tie rod for evidence of corrosion or contamination. If none is evident, continue with the repair. If corrosion or contamination is evident, replace the inner tie rod.

6. Remove the steering gear inner boot clamp (2).

### Installation Procedure

1. Install a new clamp (2) loosely on the inner part of the steering gear boot.
2. Apply grease from the service kit to the indicated locations.

Note: The steering gear boot must seat in the appropriate groove on the steering gear.

3. Install the steering gear boot (1) over the steering linkage inner tie rod and onto the steering gear.
4. Using CH-804 pliers crimp the inner steering gear boot clamp (1).
5. Install the steering gear outer boot clamp (2).
6. Install the steering linkage inner tie rod nut (1).
7. Install the steering linkage outer tie rod. Refer to Steering Linkage Outer Tie Rod Replacement.