For 1990-2009 cars

NEED GRAPHIC

Callout | Component Name
--- | ---
1 | Bolt Access Plug

#### Procedure

Use a plastic flat-bladed tool to remove.

2 | Rear Side Door Outside Handle Cap Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten XX N·m(XX lb ft)
3 | Rear Door Outside Handle Cap
4 | Rear Door Outside Handle

#### Procedure

Pull the outside handle rearward to release it from the handle housing.

5 | Rear Door Outside Handle Gasket

#### Procedure

Inspect the lock and handle adjustments. Refer to Rear Side Door Outside Handle Rod Adjustment.