For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. It is only necessary to lower the headliner. Only perform the steps in the headliner replacement procedure that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement.
2. Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.

1 | Sunroof Housing Front Drain Hose

#### Procedure

Disengage the sunroof drain hose from the attachment points on the windshield pillar.