For 1990-2009 cars

### Removal Procedure

1. Remove battery. Refer to Battery Replacement.
2. Unclip all wiring harness from battery tray.
3. Unclip the engine control module bracket from battery tray.
4. Remove the 3 battery tray bolts (1).
5. Remove the battery tray (2).

### Installation Procedure

1. Install the battery tray (3).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 3 battery tray bolts (1) and tighten to 15 N·m (11 lb ft).
3. Clip in all wiring harness at the battery tray.
4. Install battery. Refer to Battery Replacement.