For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tail lamps. Refer to Tail Lamp Replacement.

1 | Rear Bumper Fascia Retainer (Qty: 2)
2 | Rear Wheelhouse Liner Bolt (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (23 lb in)
3 | Rear Bumper Fascia

#### Procedure

1. Unclip from rear bumper fascia guides.
2. Pull forward to remove the rear bumper fascia.
3. Disconnect any electrical connectors.
4. Transfer parts as needed.