For 1990-2009 cars

Checks | Causes
--- | ---
2-6 Clutch Assembly |

• | Inspect for worn or improper surface finish on the 2-6 Clutch Plates (540-542)

• | Inspect for fatigued 2-6 Clutch Piston Apply Plate (540)

• | Inspect for plugged, restricted or incorrect orientation of the 2-6 Clutch Piston (535) air bleed

Case Assembly (50) |

• | Inspect for damaged or broken 2-6 Clutch Piston (535) and piston seals damaged, worn or delaminating

• | Inspect for fatigued 2-6 Clutch Piston Return Spring (536)