For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid. Refer to Rear Compartment Lid Replacement

1 | Rear Compartment Lid Rear Hinge Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m(80 lb in)
2 | Rear Compartment Lid Rear Hinge

#### Procedure

Adjust rear compartment lid as needed. Refer to Rear Compartment Lid Adjustment.