For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. It is only necessary to lower the headliner. Only perform the steps in the headliner replacement procedure that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement.
2. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
3. Remove the body side trim panel left side. Refer to Body Side Trim Panel Replacement - Left Side.
4. Remove the body side trim panel right side. Refer to Body Side Trim Panel Replacement - Right Side.

1 | Sunroof Housing Rear Drain Hose

#### Procedure

Disengage the sunroof drain hose from the attachment clips on the roof rail, the C-pillar, and the rear compartment.