For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transmission front mount bolt (1).
3. Remove the transmission front mount bolts (1).
4. Remove the transmission front mount (2).

### Installation Procedure

1. Install the transmission front mount (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission front mount bolts (1) and tighten to 62 N·m (46 lb ft).
3. Install the transmission front mount bolt (1) and tighten to 58 N·m (43 lb ft).
4. Lower the vehicle.