For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove rear compartment lid. Refer to Rear Compartment Lid Replacement

#### Special Tools

BO-125 Torque Rod Lifter

For equivalent regional tools, refer to Special Tools

1 | Rear Compartment Lid Hinge Torque Rod - Right Side Note: Only use the special tool to remove and install the Rear compartment lid hinge torque rod.
2 | Rear Compartment Lid Hinge Torque Rod - Left Side Note: Only use the special tool to remove and install the Rear compartment lid hinge torque rod.