For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position Sensor Fastener | 10 N·m | 89 lb in
Air Cleaner Housing Cover Bolt | 5 N·m | 44 lb in
Air Cleaner Outlet Front Duct Clamp | 3.5 N·m | 31 lb in
Air Cleaner Outlet Rear Duct Clamp | 3.5 N·m | 31 lb in
Camshaft Position Sensor Bolt | 6 N·m | 54 lb in
Crankshaft Position Sensor Fastener | 4.5 N·m | 40 lb in
Drivetrain and Front Suspension Frame Rear Bolt | 90 N·m+128° | 67 lb ft+128°
Engine Coolant Fan Bolt | 4 N·m | 36 lb in
Engine Coolant Temperature Sensor Fastener | 35 N·m | 26 lb ft
Evaporative Emission Canister Purge Solenoid Valve Bracket Bolt | 8 N·m | 71 lb in
Exhaust Pipe Front Hanger bolts | 20 N·m | 15 lb ft
Fuel Tank Filler Hose Clamp | 3 N·m | 27 lb in
Fuel Tank Filler Pipe Bracket Bolt | 9 N·m | 80 lb in
Fuel Tank Filler Pipe Ground Bolt | 9 N·m | 80 lb in
Fuel Tank Strap Bolts | 23 N·m | 17 lb ft
Heated Oxygin Sensor | 40 N·m | 30 lb ft
Ignition Coil Bolts | 8 N·m | 71 lb in
Intake air Duct Bolt | 5 N·m | 44 lb in
Knock Sensor Bolt | 20 N·m | 15 lb ft
Manifold Absolute Pressure Sensor Bolt | 1.8 N·m | 16 lb in
Multiport Fuel Injection Fuel Rail Bolt | 8 N·m | 71 lb in
Spark Plug | 25 N·m | 19 lb ft
Throttle Body Bolt | 8 N·m | 71 lb in