For 1990-2009 cars

# Driver Information and Entertainment

## All Description and Operation

- Audible Warnings Description and Operation
- Driver Information Center (DIC) Description and Operation
- Indicator/Warning Message Description and Operation
- Instrument Cluster Description and Operation

## Diagnostic Procedures

- Charge Indicator Malfunction
- Chime Malfunction
- Driver Information Center (DIC) Switch Malfunction
- Engine Oil Pressure Indicator Malfunction
- Fuel Gage Inaccurate or Inoperative
- Instrument Cluster Gages Inoperative
- Odometer Trip/Reset Switch Inoperative
- Outside Air Temperature Display Inaccurate or Inoperative
- Symptoms - Displays and Gages

## Diagnostic Trouble Codes

- DTC B0158
- DTC B0550
- DTC B3567
- DTC P0461-P0463
- DTC P0520

## Electrical/Electronic Schematic Diagrams

- Driver Information System Schematics
- Instrument Cluster Schematics

## Electrical/Electronic Specifications

- Ambient Air Temperature Sensor Resistance

## Mechanical Specifications

- Fastener Tightening Specifications

## Removal, Installation, and Replacement

- Ambient Air Temperature Gage Sensor Replacement
- Driver Information Display Replacement
- Instrument Cluster Replacement