For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Drivetrain and Front Suspension Frame Bolt Front

- First Pass

120 N·m

89 lb ft

- Final Pass

+ 128 °

Drivetrain and Front Suspension Frame Bolt Rear

- First Pass

90 N·m

67 lb ft

- Final Pass

+ 128 °

Front Compartment Insulator Bolt | 3 N·m | 27 lb in
Front Compartment Splash Shield Bolt | 3 N·m | 27 lb in
Front Wheelhouse Liner Bolt | 2.5 N·m | 23 lb in
Power Steering Fluid Cooling Pipe Bolt | 9 N·m | 80 lb in
Power Steering Inlet and Outlet Hose Bolt | 11 N·m | 98 lb in
Rear Wheelhouse Liner Bolt | 2.5 N·m | 23 lb in
Steering Linkage Tie Rod Nut | 35 N·m | 26 lb ft
Transmission Front Mount Bolt | 100 N·m | 43 lb ft
Transmission Rear Mount Bracket Bolt | 100 N·m | 74 lb ft