For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disconnect battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove instrument outer trim cover - left side. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.
3. Remove instrument panel lower trim pad cover - left side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
4. Remove floor air outlet duct - left side. Refer to Floor Air Outlet Duct Replacement - Left Side.
5. Remove radio cooling duct - left side. Refer to Radio Cooling Duct Replacement.

1 | Temperature Valve Actuator Wiring Harness

#### Procedure

Disconnect the wiring harness plug.

2 | Temperature Valve Actuator Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (23 lb in)
3 | Temperature Valve Actuator

#### Procedure

For recalibration the temperature valve actuator, refer to Temperature Valve Actuator Replacement.