For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove floor air outlet duct - left side. Refer to Floor Air Outlet Duct Replacement - Left Side.

1 | Disconnect Inside Air Temperature Sensor Wiring Harness Plug Tip The graphic shows the instrument panel compartment without instrument panel lower trim pad cover and radio cooling duct for better clarity.
2 | Inside Air Temperature Sensor

#### Procedure

Rotate the inside air temperature sensor to remove.