For 1990-2009 cars

1. Inspect the control solenoid (w/body and TCM) valve assembly connectors and pins (1, 2, 4, 6) for the following conditions:

• | Damage

• | Bent pins

• | Debris

• | Broken retaining tab

• | Contamination

2. Ensure no metallic debris is inside the connectors near the terminal pins.
3. Inspect the control solenoid (w/body and TCM) valve assembly solenoid leads (3) for contamination or metallic debris.
4. Inspect the 2 control solenoid (w/body and TCM) valve assembly filter plate retaining tabs (5) for cracks and ensure proper tension when filter plate is attached.