For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 1-2-3-4 Clutch Backing Plate Retainer Ring Warning: The retainer is under tension. Use care when removing or installing the retainer. Personal injury could result. Caution: Use caution during removal or installation of the retainer ring to avoid damage to the case machined surface in the park pawl area. Burrs or raised edges on the case machined surface can cause the park pawl to bind and prohibit it from engaging the park gear.

Tip
Remove one end of the retainer using DT-28585 snap ring remover or equivalent and work the retainer out of the case groove.

#### Special Tool

DT-28585 Snap Ring Remover or equivalent

For equivalent regional tools, refer to Special Tools.

2 | 3-5 Reverse and 4-5-6 Clutch Housing Assembly, Gearset, Low-Reverse Clutch Assembly and Low-Reverse and 1-2-3-4 Clutch Housing Tip This unit is heavy - weighs 40 lbs. (18 Kg).
3 | 2-6 Clutch Plate (Qty: 1)
4 | 2-6 Clutch Apply Plate (Waved)
5 | 35R and 456 Clutch Housing Thrust Bearing Assembly