For 1990-2009 cars

### Removal Procedure

1. Disconnect the clutch pedal position sensor wiring harness plug.
2. Remove the clutch pedal position sensor bolt (2).
3. Remove the clutch pedal position sensor (1).

### Installation Procedure

1. Install the clutch pedal position sensor (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the clutch pedal position sensor bolt (2) and tighten to xx N·m(xx lb ft).
3. Connect the clutch pedal position sensor wiring harness plug.