For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Remove the front floor console. Refer to Front Floor Console Replacement.
3. Disconnect the electrical connector.

1 | Inflatable Restraint Sensing and Diagnostic Module Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Inflatable Restraint Sensing and Diagnostic Module Assembly

#### Procedure

If installing a replacement module, program the module. Refer to Control Module References.