For 1990-2009 cars

Checks | Causes
--- | ---
Differential Carrier Assembly (232) |

• | Inspect for damaged or broken Front Differential Assembly (232)

• | Inspect for damaged or broken Front Differential Side Gear or Pinion Gear

• | Inspect for damaged or broken Front Differential Pinion Gear Shaft

• | Inspect for damaged or broken Front Differential Pinion Gear Shaft Pin

Output Carrier Transfer Drive Gear Hub Assembly (222) |

• | Inspect for broken Drive Gear Hub (222)

• | Inspect for worn, stripped or sheared Drive Gear hub (222) splines

• | Inspect for disengaged or broken Park Gear Retainer Ring (220)

• | Inspect for damaged or broken park Gear (221)

• | Inspect for disengaged or broken Drive Sprocket Retainer Ring (227)

Reaction Carrier Assembly (567) | Inspect for worn, stripped or sheared splines
Drive Link Assembly (225) |

• | Inspect for broken, worn or damaged Drive Link Assembly (225)

• | Inspect for broken, worn or damaged Drive Sprocket (224)

• | Inspect for broken, worn or damaged Driven Sprocket Assembly (229)

• | Inspect for broken Drive Gear Hub (222)

Case Assembly (50) |

• | Inspect for broken or damaged Case

• | Inspect for broken or bent Park Pawl Shaft (600)

• | Inspect for broken or missing Park Pawl Actuator Guide Pin (603) or Manual Shaft Pin (611)

• | Inspect for broken or missing Manual Shaft Detent Lever Pin (610)

• | Inspect for broken or missing Manual Shift Shaft Pin (611)

• | Inspect for damaged or broken Manual Shift Detent Lever Shaft (608)

• | Inspect for loose, damaged or broken Detent Lever Spring Assembly (17)

• | Inspect for broken, loose or misaligned Park Pawl Actuator Guide (606)

• | Inspect for binding, bent or broken Park Pawl (602) or Actuator Assembly (607)