For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement
2. Disconnect electrical from the rear object sensor.
3. Lift the locking tabs on the housing and remove the rear object sensor.

### Installation Procedure

1. Insert the sensor into the housing.
2. Connect the electrical connector to the rear object sensor.
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.