For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 3-5 Reverse and 4-5-6 Clutch Housing Thrust Bearing
2 | 2-6 Clutch Apply Plate (Waved)
3 | 2-6 Clutch Plate (Qty: 1) Tip

• | Only install one 2-6 Clutch Plate. The remaining clutch plate is installed with the gearset assembly.

• | Align the large flat areas with the valve body end of the case and the 2 tabs on the clutch plate that are close to each other with the slots at the bottom right corner of the case.

4 | 3-5 Reverse and 4-5-6 Clutch Housing Assembly and Gearset Tip Align the large flat areas of the 2-6 Clutch Plate with the valve body end of the case and the 2 tabs on the clutch plate that are close to each other with the slots at the bottom right corner of the case.