For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | Disconnect Rear Compartment Lid Wiring Harness Plug

#### Procedure

1. Disconnect the battery.
2. Release the locking device to disconnect the wiring harness plug.

2 | Rear Compartment Lid Wiring Harness