For 1990-2009 cars

## Exhaust Heat Shield Replacement 1.6L LXV

### Removal Procedure

1. Open the hood.
2. Remove the wiring harness bracket bolt (2) and the wiring harness bracket (1).
3. Remove the 2 exhaust manifold heat shield bolts (4).
4. Remove the exhaust manifold heat shield (3).

### Installation Procedure

1. Install the exhaust manifold heat shield (3).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 exhaust manifold heat shield bolts (4) and tighten to 8 N·m (71 lb in).
3. Install the wiring harness bracket (1) and the 3 bolts (2) and tighten to 15 N·m (11 lb ft).
4. Close the hood.

## Exhaust Heat Shield Replacement 2L Diesel LLW

Callout | Component Name
--- | ---
Warning: Refer to Exhaust Service Warning in the Preface section. Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

#### Preliminary Procedure

Remove the exhaust flexible pipe. Refer to Exhaust Flexible Pipe Replacement.

1 | Heat Shield Retainer (Qty: 7)
2 | Heat Shield