For 1990-2009 cars

### Removal Procedure

1. Remove the manual transmission. Refer to Transmission Replacement.
2. Remove the engine flywheel. Refer to Engine Flywheel Removal.
3. Remove the clutch pressure and driven plate. Refer to Clutch Pressure and Driven Plate Replacement.

### Installation Procedure

1. Install the clutch pressure and driven plate. Refer to Clutch Pressure and Driven Plate Replacement.
2. Install the engine flywheel. Refer to Engine Flywheel Installation.
3. Install the manual transmission. Refer to Transmission Replacement.