For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | Rear Compartment Lid Hinge Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten xx N·m (xx lb ft)
2 | Rear Compartment Lid

#### Procedure

1. Disconnect the electrical connector.
2. Adjust rear compartment as needed. Refer to Rear Compartment Lid Adjustment.
3. Transfer components as necessary.