For 1990-2009 cars

Table 1: | Digital Audio Broadcast Scan Tool Parameters
Table 2: | Digital Audio Broadcast Detection Module Output Controls

#### Digital Audio Broadcast Scan Tool Parameters

Parameter | Expected Value | Definition
--- | --- | ---
Operating Conditions: Ignition ON
Antenna Signal Strength | Varies | The scan tool displays the Antenna Signal Strength in dBm.
End Model Part Number | Varies | The scan tool displays the End Model Part Number.
Base Model Part Number | Varies | The scan tool displays the Base Model Part Number.
End Model Part Number Alpha Code | Varies | The scan tool displays the End Model Part Number Alpha Code.
Diagnostic Data Identifier | Varies | The scan tool displays the Diagnostic Data Identifier.
Vehicle Identification Number (VIN) | Varies | The scan tool displays the Vehicle Identification Number (VIN).
Mechanical Key Code | Varies | The scan tool displays the Mechanical Key Code.
Module Diagnostic Address | Varies | The scan tool displays the Module Diagnostic Address.
Date Programmed | Varies | The scan tool displays the Date Programmed.

#### Digital Audio Broadcast Detection Module Output Controls

Scan Tool Output Control | Description
--- | ---
Audio Tone | This output controls a test tone (1 kHz sinus) on left and right audio channels in order to check the audio between the Digital Audio Broadcast Module and the radio. Pressing left button a tone with 1 KHz can be heard out off the left speakers. Pressing right button a tone with 1 KHz can be heard out off the right speaker.
CAN Bus Configuration Learn | This output control will enable the module to learn the serial data speed and adapt to it.