For 1990-2009 cars

## Clutch Actuator Cylinder Replacement D16

### Removal Procedure

1. Remove the manual transmission. Refer to Transmission Replacement.
2. Detach the clutch actuator cylinder pipe (3) from the clutch actuator cylinder (2).
3. Remove the clutch actuator cylinder bolts (1).
4. Remove the clutch actuator cylinder (1).
5. Remove the clutch actuator cylinder seal (2).

### Installation Procedure

1. Install the clutch actuator cylinder seal (2).
2. Install the clutch actuator cylinder (1).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the clutch actuator cylinder bolts (1) and tighten to 7 N·m(62 lb in).
4. Attach the clutch actuator cylinder pipe (3) to the clutch actuator cylinder (2).
5. Install the manual transmission. Refer to Transmission Replacement.
6. Bleed the hydraulic clutch system. Refer to Hydraulic Clutch Bleeding.
7. Fill the reservoir with clutch/brake fluid up to the MAX level.

## Clutch Actuator Cylinder Replacement D33

### Removal Procedure

1. Remove the manual transmission. Refer to Transmission Replacement.
2. Detach the clutch actuator cylinder pipe (2).
3. Remove the clutch actuator cylinder bolts (1).
4. Remove the clutch actuator cylinder (1).
5. Remove the clutch actuator cylinder seal (2).

### Installation Procedure

1. Install the clutch actuator cylinder seal (2).
2. Install the clutch actuator cylinder (1).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the clutch actuator cylinder bolts (1) and tighten to 7 N·m (62 lb in).
4. Attach the clutch actuator cylinder pipe (2).
5. Install the manual transmission. Refer to Transmission Replacement.
6. Bleed the hydraulic clutch system. Refer to Hydraulic Clutch Bleeding.
7. Fill the reservoir with clutch/brake fluid up to the MAX level.