For 1990-2009 cars

Checks | Causes
--- | ---
Low and Reverse Clutch Assembly (543) |

• | Inspect for stripped or sheared internal or external splines on Low and Reverse Clutch Assembly (543)

• | Inspect for broken or disengaged retainer ring

Low and Reverse Clutch |

• | Inspect for stripped or sheared splines on Low and Reverse Clutch Plates (545-547)

• | Inspect for damaged, deformed or improper surface finish on the Low and Reverse Clutch Plates (545-547)

• | Inspect for stripped or sheared splines on Low and Reverse Clutch Backing Plate (544)

• | Inspect for worn, damaged or debonding Low and Reverse Clutch Piston Seals (550)

• | Inspect for broken or fatigued Low and Reverse Clutch Piston Return Spring (549)

Low-Reverse and 1-2-3-4 Clutch Housing (551) |

• | Inspect for disengaged or broken Low and Reverse Clutch Piston Spring Retainer (548)

• | Inspect for broken or deformed Low and Reverse Clutch Piston (550)

• | Inspect for damaged or improper surface finish in the piston bore