For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten xx N·m (xx lb ft)
2 | Rear License Plate Lamp

#### Procedure

Rotate the left corner of the lamp assembly upward and pull the right side down out from the rear bumper fascia opening.

3 | Rear License Plate Lamp Socket

#### Procedure

Rotate the lamp socket counterclockwise and remove.

4 | Rear License Plate Lamp Bulb

#### Procedure

Service the bulb, as needed.