For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel outer trim cover - right side. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.

1 | Instrument Panel Compartment Screw (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Instrument Panel Compartment Assembly

#### Procedure

Disconnect the compartment lamp.